UGR0149-000,REVA 5/26/98 Page 1 of 4

4440_Wide Jumper Settings

4440_Wide Jumper Settings

UGR0149-000,REVA 5/26/98 Page 2 of 4

Jumper Settings f or H4440W-001

Legend: IN refers to the jumper being installed across the pins indicated. OUT indicates that the jumper is removed. N/P indicates the jumper block is not populated on the board. JUMPER DEFAULT DESCRIPTION

J1 N/P Factory use only J2 IN CH3 TERMPOWER J3 IN CH2 TERMPOWER J4 IN CH1 TERMPOWER J5 IN CH0 TERMPOWER J6 IN Factory DEBUG only J7 N/P Factory use only J8 N/P Factory use only J9 IN SCSI ID 3 (MSB = 1-2) J10 IN SCSI ID 2 (MSB = 1-2) J11 IN SCSI ID 1 (MSB = 1-2) J12 IN SCSI ID 0 (MSB = 1-2) J13 N/P Factory use only J14 N/P Factory use only J15 OUT IN OUT Factory use only (pin# 1-12) VMEbus Request bit 1, out is 1 (pin# 13-14) VMEbus Request bit 0, out is 1 (pin# 15-16) J16 IN OUT IN OUT

SCSIINIT on power up, IN=Disable (pin# 1-2) MEMTEST, IN=Disable (pin# 3-4) Console Messages, IN=Disable (pin# 5-6) IN=GDB Enable on EXIT, OUT=GDB Enable on Reset (pin# 7-8) J17 OUT Factory use only J18 OUT Factory use only J19 IN FLASH*, IN=FLASH is used on download

4440_Wide Jumper Settings

UGR0149-000,REVA 5/26/98 Page 3 of 4

J20 OUT OUT IN OUT

16 bit Block Mode, IN=Disable (pin# 1-2) IN=Clear SYSFAIL after diag, OUT=Clear SYSFAIL before diag. (pin# 3-4) SCSI reset on-power-up, IN=Disable (pin# 5-6) GDB enable, IN=Enable (pin# 7-8) J21 OUT OUT OUT OUT

Load firmware from Eprom, IN=load from buffer (pin# 1-2) Monitor mode. IN=Enable (pin# 3-4) Secondary short I/O=2K. See Cougar’s manual (pin# 5-6) Secondary short I/O=2K (pin# 7-8) J22 OUT Factory use only (pin# 1-8) J23 N/P Factory use only J24 IN OUT IN Primary short I/O = 2K (pin# 1-4) Secondary Short I/O reset enable (pin# 5-6) Primary short I/O reset enable (pin# 7-8) J25 OUT VME DTACK 5ns delay tap J26 OUT VME DTACK 10ns delay tap J27 OUT Abort enable (IN=disable) J28 OUT Abort switch connector J29 OUT VME DTACK 15ns delay tap J30 IN Secondary Short I/O Address modifier, IN=29 # 2D, OUT=2D J31 OUT Factory use only (pin# 1-8) J32 OUT VME DTACK 20ns delay tap J33 IN Primary Short I/O Address modifier, IN=29 # 2D, OUT=2D J34 IN VME DTACK 25ns delay tap J35 OUT ISP connector J36-J39 N/P Primary short I/O address, see Cougar’s manual J40 N/P Factory use only J41 N/P Factory use only J42 N/P Factory use only J43-J46 N/P Secondary short I/O, see Cougar’s manual

4440_Wide Jumper Settings

UGR0149-000,REVA 5/26/98 Page 4 of 4

Contact Information Customer Suppor t

United States: Telephone: (214) 654-5555 Fax: (214) 654-5500 E-Mail: intouch@iphase.com Europe: Telephone: + 33 (0)1 41 15 44 00 Fax: + 33 (0)1 41 15 12 13

World Wide Web

http://www.iphase.com

Anonymous FTP Ser ver

ftp.iphase.com